**X-ray diffractometry of Si epilayers grown on porous silicon**

**G. Lamedica «Foreign» 1**

**M. Balucani «Foreign» 2**

**A. Ferrari «Foreign» 3**

**V. Bondarenko 4**

**V. Yakovtseva 5**

**L. Dolgyi 6**

4, 5, 6 Belarussian State University of Informatics and Radioelectronics

**Abstract.** X-ray double-crystal diffractometry was used to measure lattice deformation of porous silicon (PS) and Si epitaxial layers grown on PS. PS layers 1–10 μm in thickness and 15-65% in porosity were formed by anodization of n+-type Sb doped Si wafers in a 12% HF aqueous solution. Lattice deformations of both PS and epitaxial layers are shown to strongly depend on PS porosity. Grown on uniform PS 40–60% in porosity, the epilayers, single-crystal as they are, display high lattice deformation and defect density. Epilayers grown on two-layer PS are comparable with the films grown on the n+-type single-crystal Si substrate.

**Keywords:** Porous silicon; Epilayer; X-ray diffractometry; Lattice deformation.

<http://dx.doi.org/10.1016/S0921-5107(01)00997-7>

<http://www.sciencedirect.com/science/article/pii/S0921510701009977>